Parsing Interface Descriptor for device: 001/017
 iManufacturer: Dell
 iProduct: Dell Smart Card Reader Keyboard
 bLength: 9
 bDescriptorType: 4
 bInterfaceNumber: 1
 bAlternateSetting: 0
 bNumEndpoints: 3
 bInterfaceClass: 0x0B [Chip Card Interface Device Class (CCID)]
 bInterfaceSubClass: 0
 bInterfaceProtocol: 0
 iInterface: 0
 CCID Class Descriptor
  bLength: 0x36
  bDescriptorType: 0x21
  bcdCCID: 1.00
  bMaxSlotIndex: 0x00
  bVoltageSupport: 0x07
   5.0V
   3.0V
   1.8V
  dwProtocols: 0x0000 0x0003
   T=0
   T=1
  dwDefaultClock: 4.000 MHz
  dwMaximumClock: 4.000 MHz
  bNumClockSupported: 0x00
  dwDataRate: 10752 bps
  dwMaxDataRate: 344086 bps
  bNumDataRatesSupported: 0
  dwMaxIFSD: 254
  dwSynchProtocols: 0x00000000
  dwMechanical: 0x00000000
   No special characteristics
  dwFeatures: 0x00010230
   Automatic ICC clock frequency change according to parameters
   Automatic baud rate change according to frequency and Fi, Di parameters
   NAD value other than 00 accepted (T=1)
   TPDU level exchange
  dwMaxCCIDMessageLength: 271 bytes
  bClassGetResponse: 0
  bClassEnveloppe: 0
  wLcdLayout: 0x0000
  bPINSupport: 0x01
   PIN Verification supported
  bMaxCCIDBusySlots: 1
