Alcormicro CCID Smart card reader drivers for Windows CE 4.1, 4.2 And 5.0.

V 1.0.0.1

I.  For End User
---------------------------
      Install the driver STEP By STEP

	1.Copy the file "AlcCcid.dll" to "My Computer\Windows" or "My device\Windows"
	2.Attach the Card reader to your device
	3.Windows will show the dialog box, then type "alcccid"
	4.Press OK

	
II. Test program
---------------------------
   AlcorCeAP.exe is used to check  driver running correctly.
  	a)click the "Find Reader" to detect the card reader
	b)insert the ic card then press the "Check Card" 
		The program should return the ATR string if successful
	c)(optional)Some ic card may not support to "Read SN" , and card reader still will work successful. 


III. Platform Builder notes
---------------------------
  To build the os image include the driver for alcromicor 9520 card reader ,the following feature must add to the project
	1.USB Host (UHCI)
	2.SmartCard Component - SCM Microsystems SCR300 - USB Smart Card Reader

  There is two methods to add driver to CEPC
	1.Remote File viewer
	2.Add command in project.bib
  	  2.1 Click ParameterView and Project Specific Files
	  2.2 Open project.bib
          2.3 Add the following command in "Files" section - "AlcCcid.dll   (Path of the driver)\AlcCcid.dll  NK  SHC"

	3.Add command in platform.reg
          3.1 Click ParameterView and Hardware Specific Files    
	  3.2 Open platform.reg
	  3.3 Add the following command -  #include "(Path of the registy file)\AlcCcid.reg" 




-----------------------------
