PCSCD(8)

NAME
pcscd - PC/SC Smart Card Daemon

SYNOPSIS
pcscd [options]

OPTIONS

-a, --apdu
    log APDUs and SW using the debug method (see -d)

-c, --config file
    Specifies the file file as an alternate location for @confdir@/reader.conf

-d, --debug OUTPUT
    display debug messages. OUTPUT may be:
     stdout (imply --foreground),
     stderr (imply --foreground),
     or syslog

-f, --foreground
    Runs pcscd in the foreground (imply --debug stdout)

-h, --help
    Displays information about the pcscd command line

-v, --version
    Displays the program version number

DESCRIPTION
pcscd is the daemon program for pcsc-lite and the MuscleCard framework. It is a resource manager that coordinates communications with smart card readers and smart cards and cryptographic tokens that are connected to the system. pcscd is normally started at boot time from /etc/init.d/pcscd. It allows applications to access smart cards and readers without knowing details of the card or reader. pcscd coordinates the loading of drivers for card readers and plug-ins for different card types. The purpose of pcsc-lite is to provide both a cross compatible API for migrating Windows based PC/SC applications to Unix and to provide a pluggable architecture for supporting smart cards and cryptographic tokens through high level API's. At startup, pcscd loads the smart card reader drivers specified in the @confdir@/reader.conf file (or specified using -c file). When a smart card is inserted into a reader, pcscd uses the ATR string from the card to identify this card. The @muscledropdir@ directory contains plug-ins for the card. These plug-ins are searched. If the ATR string matches, the client library loads that plug-in for that token.

SERIAL SMART CARD READER DRIVERS
Smart card reader drivers are placed in the @usbdropdir@ directory. Each driver is simply an .so file. The pcscd locates the driver with the @confdir@/reader.conf file. The file has the following format:
 # comment
 FRIENDLYNAME <Descriptive name>
 DEVICENAME <Short name>
 LIBPATH <Location of the driver library>
 CHANNELID <Channel identifier>

FRIENDLYNAME
    is a user friendly name of the reader that is served by this driver. This name is displayed to the user when necessary.

DEVICENAME
    is a driver specific value. If you do not know this value, GEN_SMART_RDR is a good choice.

LIBPATH
    is the full path to the shared library.

CHANNELID
    is the channel ID for serial port smart card readers. This could vary depending on the driver in which you are using - check the driver README for more information. Some use the following:
     /dev/ttyS0 (COM1) -> 0x0103F8 or 1
     /dev/ttyS1 (COM2) -> 0x0102F8 or 2
     /dev/ttyS2 (COM3) -> 0x0103E8 or 3
     /dev/ttyS3 (COM4) -> 0x0102E8 or 4

Example:
 # Configuration file for pcsc-lite

 FRIENDLYNAME "My Smart Card Reader"
 DEVICENAME GEN_SMART_RDR
 LIBPATH @usbdropdir@/my_reader.so
 CHANNELID 0x0103F8

 # End of file Multiple drivers can be listed in @confdir@/reader.conf. Drivers are available at http://www.musclecard.com/drivers.html.

SMART CARD PLUG-INS
pcsc-lite uses plug-ins to handle different types of smart cards. There is a plug-in for each smart card type. Plug-ins are installed in the @muscledropdir@ directory. Plug-ins for cards/tokens are available from the MUSCLE web site http://www.musclecard.com/.

FILES
@confdir@/reader.conf : Reader configuration file /etc/init.d/pcscd : pcscd startup script @runpid@ : process id of the running pcscd @usbdropdir@ : directory containing bundles for USB drivers

BUGS
None known.

SEE ALSO
bundleTool(8), formaticc(1)

AUTHORS
David Corcoran <corcoran@musclecard.com> and Ludovic Rousseau <ludovic.rousseau@free.fr>